2022\_mc\_58

Task1:Use electricity to control the position of the dual acting cylinder using electrically operated directional control valve and proximity sensor

